**Sheen Zar Agriculture Trading Company**

**REQUEST FOR QUOTATION (RFQ)**  
**Procurement, Delivery and Installation of Concrete I-Trellis Kits for High-Density Vineyards and Orchards**

**RFQ Reference Number: SZATC/2025/RFQ/001**

**TABLE OF CONTENTS**

1. Provisional Timetable
2. Introduction
3. Purpose of this RFQ
4. Submission of Quotations
5. Mandatory Requirements
6. Evaluation and Award Criteria
7. RFQ Queries and Clarifications
8. Conflict of Interest
9. Payment Terms
10. Quantity Requirements

**1. PROVISIONAL TIMETABLE**

|  |  |
| --- | --- |
| Activity | Date |
| RFQ Issuance | 22 April 2025 |
| Deadline for Supplier Queries | 24 April 2025 |
| Responses to Queries | 25 April 2025 |
| Quotation Submission Deadline | 30 April 2025 |
| Quotation Opening and Evaluation | 1 May 2025 |
| Contract Award | 5 May 2025 |
| Contract Start Date | 10 May 2025 |

**2. INTRODUCTION**

Sheen Zar Agriculture Trading Company invites qualified local concrete producers and construction companies registered in Afghanistan to submit quotations for supplying concrete I-Trellis Kits for high-density vineyards and orchards.

**Priority will be given to local companies based in respective provinces or zones.**

**3. PURPOSE OF THIS RFQ**

To procure concrete I-Trellis kits conforming strictly to technical specifications provided, ensuring timely delivery and installation in specified districts and provinces across Afghanistan.

### 3.1. TECHNICAL SPECIFICATIONS (I-Trellis Kit)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| No. | Item | Description | Unit | Quantity per Jerib |
| 1 | Concrete trellis post | Concrete trellis post (4 metal wires, 8 mm diameter, with 8 hooks), 10 cm diameter x 3.7 m length with five holes, first hole 30 cm above soil surface, top hole 10 cm down from top, Concrete M20(1:1.5:3), gravel max. 12.5 mm, spacing between holes 65 cm for 3 mm wire, 17 rows, 8 posts per row. | Piece | 136 |
| 2 | Hot galvanized wire | Hot galvanized wire 3 mm diameter | Kg | 150 |
| 3 | End T-bar | End T-bar rod 50 cm diameter, 50 cm length, 3 wires 5 mm diameter, 3 hooks, center hook 16 mm iron, Concrete M20(1:1.5:3), gravel max. 12.5 mm | Piece | 34 |
| 4 | Gripple | Gripple wire joiner | Piece | 170 |
| \*\*\*Total 197 Jerib of land x 136 Trellis = 26792 | | | | |

**4. SUBMISSION OF QUOTATIONS**

* All documents must be signed and stamped.
* Quotations must be submitted via email: [quote@sheenzar.com](mailto:quote@sheenzar.com)

**Subject line = "Quotation for RFQ Number: SZATC/2025/RFQ/001"**

**Deadline:** On or before 11:00 AM, 30 April 2025

Late submissions will not be considered.

**5. MANDATORY REQUIREMENTS**

Bidders must submit:

* Valid Company Registration
* Tax Identification Document

Non-submission of these mandatory requirements will result in exclusion.

**6. EVALUATION AND AWARD CRITERIA**

* Preference given to suppliers based on provincial or zonal proximity.
* Evaluation will be based on:

| **Criteria** | **Weight (%)** |
| --- | --- |
| Price Competitiveness | 60% |
| Technical Capability & Experience | 20% |
| Delivery Time | 10% |
| Local Presence/Province | 10% |

**7. RFQ QUERIES AND CLARIFICATIONS**

Queries should be emailed by 30 April 2025 to:

[**quote@sheenzar.com**](mailto:quote@sheenzar.com)

**8. CONFLICT OF INTEREST**

Suppliers must declare any potential or actual conflicts of interest. Failure to disclose conflicts may lead to disqualification.

**9. PAYMENT TERMS**

* Payments through bank transfer within 21 days of successful delivery.
* Quotations must be in AFN. Exchange rate reference: DA Afghanistan Bank.

**10. QUANTITY REQUIREMENTS**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Zone | Province | District | Trellis Qty | Unit Price | Total  Price |
| Central | Kabul | Charasyab | 952 |  |  |
| Central | Maidan Wardak | Sayedabad | 952 |  |  |
| Central | Maidan Wardak | Jalriz | 680 |  |  |
| Central Highland | Bamyan | Center | 952 |  |  |
| Central Highland | Bamyan | Yakawolang | 952 |  |  |
| Central Highland | Daikundi | Provincial Capital (Nili) | 1360 |  |  |
| Central Highland | Daikundi | Shahristan | 1224 |  |  |
| Sub-Total ZONE 1 | | | | |  |
| East | Kunar | Khas Kunar | 952 |  |  |
| East | Kunar | Asadabad | 952 |  |  |
| East | Laghman | Qarghaee | 952 |  |  |
| East | Nangarhar | Khugiani | 952 |  |  |
| East | Nuristan | Bargimatal | 1224 |  |  |
| Sub-Total ZONE 2 | | | | |  |
| North | Balkh | Balkh | 952 |  |  |
| North | Samangan | Aybak | 952 |  |  |
| North East | Badakhshan | Ishkashim | 952 |  |  |
| North East | Baghlan | Khost Wa Fering | 952 |  |  |
| North East | Baghlan | Andarab | 952 |  |  |
| North East | Takhar | Farkhar | 952 |  |  |
| Sub-Total ZONE 3 | | | | |  |
| South East | Ghazni | Ghazni center | 952 |  |  |
| South East | Ghazni | Andar | 952 |  |  |
| South East | Khost | Nadersha Kot | 680 |  |  |
| South East | Khost | Musakhil | 680 |  |  |
| South East | Paktika | Ziruk | 952 |  |  |
| South East | Paktika | Mata Khan | 952 |  |  |
| South East | Paktiya | Rohani Baba | 952 |  |  |
| South East | Paktiya | Gardiz | 952 |  |  |
| Sub-Total ZONE 4 | | | | |  |
| West | Ghor | Firoozkoh | 952 |  |  |
| West | Ghor | Saghar | 952 |  |  |
| Sub-Total ZONE 5 | | | | |  |
| TOAL | | | | |  |

**Authorized by:**  
Sheen Zar Agriculture Trading Co.  
Kabul, Afghanistan  
22 April 2025